vzmodel=0 			# 0 = VZ200, 1 = VZ300			
display=0 			# 0 = PAL, 1 = NTSC
gfx=1 				# 0 = normal, 1 = australian, 2 = german
external_font=0 		# 0 = disabled, 1 = enabled
snow=0 				# 0 = none, 1 = 6847 artefacts
monitor=1 			# 0 = monochrome, 1 = colour
inverse=0			# inverse hires 256x192 colours
disk_drives=1 			# 0 or 1. If 1, the cartfile should be vzdos.rom 
joystick=0 			# 0 or 1
rom_writes=0 			# 1 = allow POKEs to ROM mem
cartridge_writes=0 		# 1 = allow POKEs to Cart mem
synchVZ=1 			# lock speed at 50 fps
cassetteAudio=1 		# play cassette tones when loading or saving
diskAudio=1 			# play stepper motor sound 
top_of_memory=65535  		# 36863=8k 47103=18k 53247=24k 63487=34k 65535=64k 5=4meg 
fast_load=1			# 1 = dont display snapshot details after load
romFile=roms\vzrom.v21  	# path of main rom 
cartFile=NONE		 	# path of cartridge rom, or NONE 
fontFile=NONE 			# path of external font file, or NONE 

#
#	Default RGB colour values for VZ palette. Format is 0xRRGGBB in hex
#	Adjust to match the colour settings of your real VZ/TV combo
#	Or experiment to apply B&W/Green/Amber monitor filter
#

RGB_Green=0x00ff00 
RGB_Yellow=0xffff00 
RGB_Blue=0x0000ff 
RGB_Red=0xff0000 
RGB_Buff=0xffffff 
RGB_Cyan=0x00ffff 
RGB_Magenta=0xff00ff 
RGB_Orange=0xff8000 
RGB_Black=0x000000 
RGB_DarkGreen=0x006000 
RGB_BrightGreen=0xa0a0a0 
RGB_DarkOrange=0x401000 
RGB_BrightOrange=0xffc418 
